PGW VERZE = 3.0.038
DRIVER = "ELSACO PROMOS-PL2"
OVLADAC
END
GROUP SK1
  TITLE = "SK1"
  ICON = "BITMAPY\SK1.BMP"
  SCREEN OBR1
    TITLE = "OBR1"
    ICON = "BITMAPY\OBR1.BMP"
    MODULES
      A_CCPU21.1,105,284
        com0 na OUT,A_SCRIN.3
        com1 na OUT,A_SCRIN.5
        com2 na OUT,A_SCRIN.4
        priorita =   0
        rychlost =   3
        filter =  10
        Hmez0 =      100.00
        Dmez0 =        0.00
        korekce0 =        0.00
        Hmez1 =      100.00
        Dmez1 =        0.00
        korekce1 =        0.00
        Hmez2 =      100.00
        Dmez2 =        0.00
        korekce2 =        0.00
        Hmez3 =      100.00
        Dmez3 =        0.00
        korekce3 =        0.00
        Hmez4 =      100.00
        Dmez4 =        0.00
        korekce4 =        0.00
        Hmez5 =      100.00
        Dmez5 =        0.00
        korekce5 =        0.00
        OVLADAC
          P2_USER Linearisation = "00000000"
          P2_USER Counter_switch = "00000000"
          P2_USER PRIORITY = 1
        END
      END
      A_CKDM_________11.1,288,35
        backlight na 3,A_Constl.1
        priorita =   0
        rychlost =   3
        address =   2
        noterm =   0
        access =   0
        OVLADAC
          P2_USER PRIORITY = 1
        END
      END
      A_Systemovy___monitor.1,519,69
        menu na scf1,A_CKDM_________11.1
        priorita =   0
        rychlost =   2
        version =        0
        CRC =        0
        pwtout =    10
        address =  1
        memory =  0
        loop1 =  0
        loop2 =  0
        loop3 =  0
        outlock =  0
        writecheck =  0
        erase_error =  0
        overdrive =     0
      END
      A_SerialComm.1,392,276
        strobe na bin0,A_CCPU21.1
        8 na out,A_Scale.1
        priorita =   2
        rychlost =   2
        Baudrate =  55
        Parity =   0
        Format =  88
        Timeout =    10
        COMnr =   1
        OVLADAC
          P2_USER Message_tx_format0 = "22303754b510D"
          P2_USER Message_tx_format1 = ""
          P2_USER Message_rx_format0 = "2130370D"
          P2_USER Message_rx_format1 = ""
          P2_USER PRIORITY = 1
        END
      END
      A_Screen.1,435,21
        11 na sc,A_CKDM_________11.1
        13 na out,A_Scale.1
        priorita =   0
        rychlost =   3
        prehlidka =   1
        access =   0
        enb_kask =   0
        edit0init =        0.00
        edit1init =        0.00
        edit2init =        0.00
        edit3init =        0.00
        dispedit =    0
        OVLADAC
          P2_USER Text_line_0 = "#T"
          P2_USER Text_line_1 = ""
          P2_USER Text_line_2 = "Voda: ###.#5"
          P2_USER Text_line_3 = "ZALOHA SW"
          P2_USER Text_line_4 = "Line4"
          P2_USER Text_line_5 = "Line5"
          P2_USER Text_line_6 = "Line6"
          P2_USER Text_line_7 = "Line7"
          P2_USER PRIORITY = 1
        END
      END
      A_SCROUT.1,464,348
        POPIS = "sc2"
        IN na error,A_SerialComm.2
      END
      A_SCROUT.3,465,282
        POPIS = "ScomErr"
        IN na error,A_SerialComm.1
        FIX
      END
      A_Flag.1,350,466
        erase na bin5,A_CCPU21.1
        priorita =   0
        rychlost =   3
      END
      A_SCROUT.4,450,465
        POPIS = "Flag.1.reset"
        IN na reset,A_Flag.1
        NUM
      END
      A_SCROUT.5,459,489
        POPIS = "Flag.1.com"
        IN na com,A_Flag.1
      END
      A_SCROUT.6,459,517
        POPIS = "Flag.1.rx0"
        IN na rx0,A_Flag.1
      END
      A_SCROUT.7,459,530
        POPIS = "Flag.1.rx1"
        IN na rx1,A_Flag.1
        NUM
      END
      A_SCROUT.8,459,543
        POPIS = "Flag.1.rx2"
        IN na rx2,A_Flag.1
      END
      A_SCROUT.9,459,556
        POPIS = "Flag.1.bat"
        IN na bat,A_Flag.1
      END
      A_Constl.1,212,98
        priorita =   0
        rychlost =   1
        hodnota =          1
        OVLADAC
          P2_USER PRIORITY = 1
        END
      END
      A_SCROUT.10,604,228
        POPIS = "Err"
        IN na error,A_Systemovy___monitor.1
        FIX
      END
      A_SCRIN.3,22,348
        POPIS = "Err"
        FIX
      END
      A_SCRIN.4,22,374
        POPIS = "sc2"
        FIX
      END
      A_SCRIN.5,22,361
        POPIS = "ScomErr"
        FIX
      END
      A_Scale.1,208,346
        in na ain1,A_CCPU21.1
        priorita =   0
        rychlost =   3
        outhipar =      100.00
        inhipar =       10.00
        inlopar =        0.00
        outlopar =        0.00
      END
      A_SerialComm.2,393,342
        strobe na bin1,A_CCPU21.1
        priorita =   1
        rychlost =   2
        Baudrate =  55
        Parity =   0
        Format =  88
        Timeout =     5
        COMnr =   1
        OVLADAC
          P2_USER Message_tx_format0 = "22303754566F64610D"
          P2_USER Message_tx_format1 = ""
          P2_USER Message_rx_format0 = "2130370D"
          P2_USER Message_rx_format1 = ""
          P2_USER PRIORITY = 1
        END
      END
      A_Flash.1,616,10
        in0 na 6,A_Screen.1
        priorita =   0
        rychlost =   3
        flash =   0
        userload =   0
        usersave =   0
      END
    END
  END
END
