PGW VERZE = 3.0.038
LOCKPOZ
DRIVER = "ELSACO PROMOS-PL2"
OVLADAC
END
GROUP SK1
  TITLE = "SK1"
  ICON = "BITMAPY\SK1.BMP"
  SCREEN OBR1
    TITLE = "OBR1"
    ICON = "BITMAPY\OBR1.BMP"
    MODULES
      A_CCPU03.1,3,121
        priorita =   0
        rychlost =   3
        OVLADAC
          P2_USER Counter_switch = "00000000"
          P2_USER PRIORITY = 1
        END
      END
      A_Systemovy___monitor.1,336,0
        menu na scf1,A_CKDM_________11.1
        priorita =   0
        rychlost =   2
        version =        0
        CRC =        0
        pwtout =    10
        address =  1
        memory =  0
        loop1 =  0
        loop2 =  0
        loop3 =  0
        outlock =  0
        writecheck =  0
        erase_error =  0
        overdrive =     0
      END
      A_CKDM_________11.1,253,20
        red1 na OUT,A_SCRIN.1
        red2 na OUT,A_SCRIN.3
        backlight na bin7,A_CCPU03.1
        priorita =   0
        rychlost =   3
        address =   2
        noterm =   0
        access =   0
        OVLADAC
          P2_USER PRIORITY = 1
        END
      END
      A_Screen.1,335,298
        11 na sc,A_CKDM_________11.1
        12 na output,A_Int2float.1
        13 na output1,A_Int2float.1
        14 na output2,A_Int2float.1
        15 na output3,A_Int2float.1
        priorita =   0
        rychlost =   3
        prehlidka =   0
        access =   0
        enb_kask =   0
        edit0init =        0.00
        edit1init =        0.00
        edit2init =        0.00
        edit3init =        0.00
        dispedit =    0
        OVLADAC
          P2_USER Text_line_0 = "#T"
          P2_USER Text_line_1 = "    test SAM-02"
          P2_USER Text_line_2 = "In3 In2 In1 In0"
          P2_USER Text_line_3 = " #7  #6  #5  #4"
          P2_USER Text_line_4 = "Line4"
          P2_USER Text_line_5 = "Line5"
          P2_USER Text_line_6 = "Line6"
          P2_USER Text_line_7 = "Line7"
          P2_USER PRIORITY = 1
        END
      END
      A_SerialComm.1,195,175
        7 na intout,A_binint.1
        priorita =   0
        rychlost =   3
        Baudrate =  66
        Parity =   0
        Format =  88
        Timeout =    10
        COMnr =   1
        OVLADAC
          P2_USER Message_tx_format0 = "403034h10D"
          P2_USER Message_tx_format1 = ""
          P2_USER Message_rx_format0 = "2130340D"
          P2_USER Message_rx_format1 = ""
          P2_USER PRIORITY = 1
        END
      END
      A_binint.1,106,124
        in0 na bin0,A_CCPU03.1
        in1 na bin1,A_CCPU03.1
        in2 na bin2,A_CCPU03.1
        in3 na bin3,A_CCPU03.1
        priorita =   0
        rychlost =   3
      END
      A_SCROUT.1,269,181
        POPIS = "SerialComm.1.error"
        IN na error,A_SerialComm.1
      END
      A_SCRIN.1,90,34
        POPIS = "SerialComm.1.error"
        FIX
      END
      A_SerialComm.2,18,396
        priorita =   0
        rychlost =   3
        Baudrate =  66
        Parity =   0
        Format =  88
        Timeout =    10
        COMnr =   1
        OVLADAC
          P2_USER Message_tx_format0 = "403034490D"
          P2_USER Message_tx_format1 = ""
          P2_USER Message_rx_format0 = "213034##h10D"
          P2_USER Message_rx_format1 = ""
          P2_USER PRIORITY = 1
        END
      END
      A_Int2float.1,277,335
        input na out0,A_Intbin.1
        input1 na out1,A_Intbin.1
        input2 na out2,A_Intbin.1
        input3 na out3,A_Intbin.1
        priorita =   0
        rychlost =   3
      END
      A_SCROUT.2,103,403
        POPIS = "iny"
        IN na 3,A_SerialComm.2
        NUM
        FIX
      END
      A_SCROUT.4,74,348
        POPIS = "SerialComm.2.error"
        IN na error,A_SerialComm.2
      END
      A_Intbin.1,199,345
        intin na 3,A_SerialComm.2
        priorita =   0
        rychlost =   3
      END
      A_SCRIN.3,90,55
        POPIS = "SerialComm.2.error"
        FIX
      END
      A_SCROUT.3,173,245
        POPIS = "binint.1.intout"
        IN na intout,A_binint.1
        NUM
      END
    END
  END
END
